# Static Call Graph for image .\Objects\project.axf

#<CALLGRAPH># ARM Linker, 5050169: Last Updated: Wed Oct 25 09:25:41 2017

### Maximum Stack Usage = 176 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ IC_test ⇒ PcdRequest ⇒ PcdComMF522 ⇒ SetBitMask ⇒ WriteRawRC ⇒ SPI_RC522_SendByte ⇒ Delay_us

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - BusFault_Handler from stm32f10x_it.o(i.BusFault_Handler) referenced from startup_stm32f10x_ld.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(i.DebugMon_Handler) referenced from startup_stm32f10x_ld.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - HardFault_Handler from stm32f10x_it.o(i.HardFault_Handler) referenced from startup_stm32f10x_ld.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - MemManage_Handler from stm32f10x_it.o(i.MemManage_Handler) referenced from startup_stm32f10x_ld.o(RESET)
  - NMI_Handler from stm32f10x_it.o(i.NMI_Handler) referenced from startup_stm32f10x_ld.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - PendSV_Handler from stm32f10x_it.o(i.PendSV_Handler) referenced from startup_stm32f10x_ld.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - Reset_Handler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - SVC_Handler from stm32f10x_it.o(i.SVC_Handler) referenced from startup_stm32f10x_ld.o(RESET)
  - SysTick_Handler from stm32f10x_it.o(i.SysTick_Handler) referenced from startup_stm32f10x_ld.o(RESET)
  - SystemInit from system_stm32f10x.o(i.SystemInit) referenced from startup_stm32f10x_ld.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - USART1_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(i.UsageFault_Handler) referenced from startup_stm32f10x_ld.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_ld.o(.text) referenced from startup_stm32f10x_ld.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f10x_ld.o(.text)
  - _printf_input_char from _printf_char_common.o(.text) referenced from _printf_char_common.o(.text)
  - _sputc from _sputc.o(.text) referenced from noretval__2sprintf.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_copy (Thumb, 26 bytes, Stack size unknown bytes, __scatter_copy.o(!!handler_copy), UNUSED)
  [Calls]

  - >> __scatterload_copy
  [Called By]
  - >> __scatterload_copy

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  _printf_percent (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent.o(.ARM.Collect$$_printf_percent$$00000000))
  [Called By]

  - >> __printf

  _printf_x (Thumb, 0 bytes, Stack size unknown bytes, _printf_x.o(.ARM.Collect$$_printf_percent$$0000000C))
  [Stack]

  - Max Depth = 64 + Unknown Stack Size
  - Call Chain = _printf_x ⇒ _printf_int_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_hex

  _printf_percent_end (Thumb, 0 bytes, Stack size unknown bytes, _printf_percent_end.o(.ARM.Collect$$_printf_percent$$00000017))

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000F))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000003))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000B))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 176 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ IC_test ⇒ PcdRequest ⇒ PcdComMF522 ⇒ SetBitMask ⇒ WriteRawRC ⇒ SPI_RC522_SendByte ⇒ Delay_us
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_ld.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_ld.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_ld.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __2sprintf (Thumb, 34 bytes, Stack size 32 bytes, noretval__2sprintf.o(.text))
  [Stack]

  - Max Depth = 136 + Unknown Stack Size
  - Call Chain = __2sprintf ⇒ _printf_char_common ⇒ __printf
  [Calls]
  - >> _sputc
  - >> _printf_char_common
  [Called By]
  - >> IC_test

  _printf_pre_padding (Thumb, 44 bytes, Stack size 16 bytes, _printf_pad.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_pre_padding
  [Called By]
  - >> _printf_int_common

  _printf_post_padding (Thumb, 34 bytes, Stack size 16 bytes, _printf_pad.o(.text))
  [Stack]

  - Max Depth = 16
  - Call Chain = _printf_post_padding
  [Called By]
  - >> _printf_int_common

  _printf_int_hex (Thumb, 84 bytes, Stack size 16 bytes, _printf_hex_int.o(.text))
  [Stack]

  - Max Depth = 64
  - Call Chain = _printf_int_hex ⇒ _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_int_common
  [Called By]
  - >> _printf_x

  _printf_longlong_hex (Thumb, 0 bytes, Stack size 16 bytes, _printf_hex_int.o(.text), UNUSED)

  __printf (Thumb, 308 bytes, Stack size 40 bytes, __printf_flags_wp.o(.text))
  [Stack]

  - Max Depth = 40 + Unknown Stack Size
  - Call Chain = __printf
  [Calls]
  - >> _printf_percent
  - >> _is_digit
  [Called By]
  - >> _printf_char_common

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  _printf_int_common (Thumb, 178 bytes, Stack size 32 bytes, _printf_intcommon.o(.text))
  [Stack]

  - Max Depth = 48
  - Call Chain = _printf_int_common ⇒ _printf_post_padding
  [Calls]
  - >> _printf_post_padding
  - >> _printf_pre_padding
  [Called By]
  - >> _printf_int_hex

  _printf_char_common (Thumb, 32 bytes, Stack size 64 bytes, _printf_char_common.o(.text))
  [Stack]

  - Max Depth = 104 + Unknown Stack Size
  - Call Chain = _printf_char_common ⇒ __printf
  [Calls]
  - >> __printf
  [Called By]
  - >> __2sprintf

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, _sputc.o(.text))
  [Called By]

  - >> __2sprintf
  [Address Reference Count : 1]
  - noretval__2sprintf.o(.text)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_perproc_libspace
  - >> __user_initial_stackheap
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 12 bytes, Stack size 0 bytes, exit.o(.text))
  [Calls]

  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  __semihosting_library_function (Thumb, 0 bytes, Stack size 0 bytes, indicate_semi.o(.text), UNUSED)

  CAN_FilterInit (Thumb, 258 bytes, Stack size 8 bytes, stm32f10x_can.o(i.CAN_FilterInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = CAN_FilterInit
  [Called By]
  - >> CAN_Mode_Init

  CAN_Init (Thumb, 276 bytes, Stack size 12 bytes, stm32f10x_can.o(i.CAN_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = CAN_Init
  [Called By]
  - >> CAN_Mode_Init

  CAN_Mode_Init (Thumb, 198 bytes, Stack size 56 bytes, can.o(i.CAN_Mode_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = CAN_Mode_Init ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_APB1PeriphClockCmd
  - >> GPIO_Init
  - >> CAN_Init
  - >> CAN_FilterInit
  [Called By]
  - >> main

  ClearBitMask (Thumb, 26 bytes, Stack size 16 bytes, rc522_function.o(i.ClearBitMask))
  [Stack]

  - Max Depth = 56
  - Call Chain = ClearBitMask ⇒ WriteRawRC ⇒ SPI_RC522_SendByte ⇒ Delay_us
  [Calls]
  - >> WriteRawRC
  - >> ReadRawRC
  [Called By]
  - >> PcdComMF522
  - >> PcdRequest
  - >> PcdAnticoll
  - >> M500PcdConfigISOType

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  Delay_us (Thumb, 52 bytes, Stack size 8 bytes, bsp_systick.o(i.Delay_us))
  [Stack]

  - Max Depth = 8
  - Call Chain = Delay_us
  [Called By]
  - >> SPI_RC522_SendByte
  - >> SPI_RC522_ReadByte
  - >> PcdReset
  - >> M500PcdConfigISOType

  GPIO_Init (Thumb, 278 bytes, Stack size 24 bytes, stm32f10x_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> RC522_SPI_Config
  - >> USART1_Config
  - >> LED_GPIO_Config
  - >> CAN_Mode_Init

  GPIO_ReadInputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_ReadInputDataBit))
  [Called By]

  - >> SPI_RC522_ReadByte

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_ResetBits))
  [Called By]

  - >> WriteRawRC
  - >> SPI_RC522_SendByte
  - >> SPI_RC522_ReadByte
  - >> ReadRawRC
  - >> PcdReset

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_SetBits))
  [Called By]

  - >> WriteRawRC
  - >> SPI_RC522_SendByte
  - >> SPI_RC522_ReadByte
  - >> ReadRawRC
  - >> RC522_Init
  - >> PcdReset
  - >> LED_GPIO_Config

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  IC_test (Thumb, 80 bytes, Stack size 16 bytes, main.o(i.IC_test))
  [Stack]

  - Max Depth = 168 + Unknown Stack Size
  - Call Chain = IC_test ⇒ PcdRequest ⇒ PcdComMF522 ⇒ SetBitMask ⇒ WriteRawRC ⇒ SPI_RC522_SendByte ⇒ Delay_us
  [Calls]
  - >> USART1_printf
  - >> PcdRequest
  - >> PcdAnticoll
  - >> __2sprintf
  [Called By]
  - >> main

  LED_GPIO_Config (Thumb, 50 bytes, Stack size 8 bytes, led.o(i.LED_GPIO_Config))
  [Stack]

  - Max Depth = 32
  - Call Chain = LED_GPIO_Config ⇒ GPIO_Init
  [Calls]
  - >> GPIO_SetBits
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  M500PcdConfigISOType (Thumb, 84 bytes, Stack size 8 bytes, rc522_function.o(i.M500PcdConfigISOType))
  [Stack]

  - Max Depth = 72
  - Call Chain = M500PcdConfigISOType ⇒ PcdAntennaOn ⇒ SetBitMask ⇒ WriteRawRC ⇒ SPI_RC522_SendByte ⇒ Delay_us
  [Calls]
  - >> Delay_us
  - >> WriteRawRC
  - >> PcdAntennaOn
  - >> ClearBitMask
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  PcdAntennaOn (Thumb, 26 bytes, Stack size 8 bytes, rc522_function.o(i.PcdAntennaOn))
  [Stack]

  - Max Depth = 64
  - Call Chain = PcdAntennaOn ⇒ SetBitMask ⇒ WriteRawRC ⇒ SPI_RC522_SendByte ⇒ Delay_us
  [Calls]
  - >> SetBitMask
  - >> ReadRawRC
  [Called By]
  - >> M500PcdConfigISOType

  PcdAnticoll (Thumb, 114 bytes, Stack size 48 bytes, rc522_function.o(i.PcdAnticoll))
  [Stack]

  - Max Depth = 152
  - Call Chain = PcdAnticoll ⇒ PcdComMF522 ⇒ SetBitMask ⇒ WriteRawRC ⇒ SPI_RC522_SendByte ⇒ Delay_us
  [Calls]
  - >> WriteRawRC
  - >> SetBitMask
  - >> PcdComMF522
  - >> ClearBitMask
  [Called By]
  - >> IC_test

  PcdComMF522 (Thumb, 306 bytes, Stack size 48 bytes, rc522_function.o(i.PcdComMF522))
  [Stack]

  - Max Depth = 104
  - Call Chain = PcdComMF522 ⇒ SetBitMask ⇒ WriteRawRC ⇒ SPI_RC522_SendByte ⇒ Delay_us
  [Calls]
  - >> WriteRawRC
  - >> SetBitMask
  - >> ReadRawRC
  - >> ClearBitMask
  [Called By]
  - >> PcdRequest
  - >> PcdAnticoll

  PcdRequest (Thumb, 86 bytes, Stack size 48 bytes, rc522_function.o(i.PcdRequest))
  [Stack]

  - Max Depth = 152
  - Call Chain = PcdRequest ⇒ PcdComMF522 ⇒ SetBitMask ⇒ WriteRawRC ⇒ SPI_RC522_SendByte ⇒ Delay_us
  [Calls]
  - >> WriteRawRC
  - >> SetBitMask
  - >> PcdComMF522
  - >> ClearBitMask
  [Called By]
  - >> IC_test

  PcdReset (Thumb, 124 bytes, Stack size 8 bytes, rc522_function.o(i.PcdReset))
  [Stack]

  - Max Depth = 48
  - Call Chain = PcdReset ⇒ WriteRawRC ⇒ SPI_RC522_SendByte ⇒ Delay_us
  [Calls]
  - >> GPIO_ResetBits
  - >> Delay_us
  - >> WriteRawRC
  - >> ReadRawRC
  - >> GPIO_SetBits
  [Called By]
  - >> main

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  RC522_Init (Thumb, 24 bytes, Stack size 8 bytes, rc522_config.o(i.RC522_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = RC522_Init ⇒ RC522_SPI_Config ⇒ GPIO_Init
  [Calls]
  - >> GPIO_SetBits
  - >> RC522_SPI_Config
  [Called By]
  - >> main

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphClockCmd))
  [Called By]

  - >> CAN_Mode_Init

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> RC522_SPI_Config
  - >> USART1_Config
  - >> LED_GPIO_Config
  - >> CAN_Mode_Init

  RCC_GetClocksFreq (Thumb, 192 bytes, Stack size 12 bytes, stm32f10x_rcc.o(i.RCC_GetClocksFreq))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init

  ReadRawRC (Thumb, 46 bytes, Stack size 16 bytes, rc522_function.o(i.ReadRawRC))
  [Stack]

  - Max Depth = 40
  - Call Chain = ReadRawRC ⇒ SPI_RC522_SendByte ⇒ Delay_us
  [Calls]
  - >> GPIO_ResetBits
  - >> SPI_RC522_SendByte
  - >> SPI_RC522_ReadByte
  - >> GPIO_SetBits
  [Called By]
  - >> SetBitMask
  - >> PcdComMF522
  - >> PcdAntennaOn
  - >> ClearBitMask
  - >> PcdReset

  SPI_RC522_ReadByte (Thumb, 72 bytes, Stack size 16 bytes, rc522_function.o(i.SPI_RC522_ReadByte))
  [Stack]

  - Max Depth = 24
  - Call Chain = SPI_RC522_ReadByte ⇒ Delay_us
  [Calls]
  - >> GPIO_ResetBits
  - >> GPIO_ReadInputDataBit
  - >> Delay_us
  - >> GPIO_SetBits
  [Called By]
  - >> ReadRawRC

  SPI_RC522_SendByte (Thumb, 80 bytes, Stack size 16 bytes, rc522_function.o(i.SPI_RC522_SendByte))
  [Stack]

  - Max Depth = 24
  - Call Chain = SPI_RC522_SendByte ⇒ Delay_us
  [Calls]
  - >> GPIO_ResetBits
  - >> Delay_us
  - >> GPIO_SetBits
  [Called By]
  - >> WriteRawRC
  - >> ReadRawRC

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  SetBitMask (Thumb, 26 bytes, Stack size 16 bytes, rc522_function.o(i.SetBitMask))
  [Stack]

  - Max Depth = 56
  - Call Chain = SetBitMask ⇒ WriteRawRC ⇒ SPI_RC522_SendByte ⇒ Delay_us
  [Calls]
  - >> WriteRawRC
  - >> ReadRawRC
  [Called By]
  - >> PcdComMF522
  - >> PcdAntennaOn
  - >> PcdRequest
  - >> PcdAnticoll

  SysTick_Handler (Thumb, 8 bytes, Stack size 8 bytes, stm32f10x_it.o(i.SysTick_Handler))
  [Stack]

  - Max Depth = 8
  - Call Chain = SysTick_Handler
  [Calls]
  - >> TimingDelay_Decrement
  [Address Reference Count : 1]
  - startup_stm32f10x_ld.o(RESET)

  SysTick_Init (Thumb, 106 bytes, Stack size 12 bytes, bsp_systick.o(i.SysTick_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = SysTick_Init
  [Called By]
  - >> main

  SystemInit (Thumb, 78 bytes, Stack size 8 bytes, system_stm32f10x.o(i.SystemInit))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f10x_ld.o(.text)

  TimingDelay_Decrement (Thumb, 18 bytes, Stack size 0 bytes, bsp_systick.o(i.TimingDelay_Decrement))
  [Called By]

  - >> SysTick_Handler

  USART1_Config (Thumb, 114 bytes, Stack size 24 bytes, usart1.o(i.USART1_Config))
  [Stack]

  - Max Depth = 92
  - Call Chain = USART1_Config ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> USART_Init
  - >> USART_Cmd
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> main

  USART1_printf (Thumb, 262 bytes, Stack size 56 bytes, usart1.o(i.USART1_printf))
  [Stack]

  - Max Depth = 76
  - Call Chain = USART1_printf ⇒ itoa
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  - >> itoa
  [Called By]
  - >> main
  - >> IC_test

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_Cmd))
  [Called By]

  - >> USART1_Config

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_GetFlagStatus))
  [Called By]

  - >> USART1_printf

  USART_Init (Thumb, 210 bytes, Stack size 56 bytes, stm32f10x_usart.o(i.USART_Init))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> USART1_Config

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_SendData))
  [Called By]

  - >> USART1_printf

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_ld.o(RESET)

  WriteRawRC (Thumb, 42 bytes, Stack size 16 bytes, rc522_function.o(i.WriteRawRC))
  [Stack]

  - Max Depth = 40
  - Call Chain = WriteRawRC ⇒ SPI_RC522_SendByte ⇒ Delay_us
  [Calls]
  - >> GPIO_ResetBits
  - >> SPI_RC522_SendByte
  - >> GPIO_SetBits
  [Called By]
  - >> SetBitMask
  - >> PcdComMF522
  - >> ClearBitMask
  - >> PcdReset
  - >> PcdRequest
  - >> PcdAnticoll
  - >> M500PcdConfigISOType

  _is_digit (Thumb, 14 bytes, Stack size 0 bytes, __printf_wp.o(i._is_digit))
  [Called By]

  - >> __printf

  main (Thumb, 68 bytes, Stack size 8 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 176 + Unknown Stack Size
  - Call Chain = main ⇒ IC_test ⇒ PcdRequest ⇒ PcdComMF522 ⇒ SetBitMask ⇒ WriteRawRC ⇒ SPI_RC522_SendByte ⇒ Delay_us
  [Calls]
  - >> USART1_printf
  - >> USART1_Config
  - >> SysTick_Init
  - >> RC522_Init
  - >> PcdReset
  - >> M500PcdConfigISOType
  - >> LED_GPIO_Config
  - >> CAN_Mode_Init
  - >> IC_test
  [Called By]
  - >> __rt_entry_main

  ### Local Symbols

  RC522_SPI_Config (Thumb, 168 bytes, Stack size 8 bytes, rc522_config.o(i.RC522_SPI_Config))
  [Stack]

  - Max Depth = 32
  - Call Chain = RC522_SPI_Config ⇒ GPIO_Init
  [Calls]
  - >> RCC_APB2PeriphClockCmd
  - >> GPIO_Init
  [Called By]
  - >> RC522_Init

  itoa (Thumb, 98 bytes, Stack size 20 bytes, usart1.o(i.itoa))
  [Stack]

  - Max Depth = 20
  - Call Chain = itoa
  [Called By]
  - >> USART1_printf

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x.o(i.SetSysClock))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  SetSysClockTo72 (Thumb, 214 bytes, Stack size 12 bytes, system_stm32f10x.o(i.SetSysClockTo72))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  _printf_input_char (Thumb, 10 bytes, Stack size 0 bytes, _printf_char_common.o(.text))
  [Address Reference Count : 1]

  - _printf_char_common.o(.text)

  ### Undefined Global Symbols